* Console cable is used to configurate swith from a console

Some commads : -

Initially switch is in user mode to change it to propagation mode use command

**Switch> enable 🡪we get switch# denoting**

From propagation mode to configuration

Switch#>config terminal 🡪Switch(Config)

Switch(Config)>hostname cse 🡪hostname is command.

Cse(config)#>exit 🡪just check it exit from config mode and we well go to propagation mode

Similary, to go into user mode run exit command again

Ok ,Now go to config mode:-

Connmad: enable password <Your password>

Exit and come again here

Command:>configurate terminal

For Secreat Password: -

Cse(config)> enable secret <your password> 🡪cse321

Now again exit and go to config mode

When entering password🡪Enter secret password

* When ever there is plain passwoed and secreat password we have to use only 🡪secret password

From propagation mode:- Run command

Cse#: 🡪 show running-config

**If we are in config mode we have to run cse(config)>do show running-config**

**Now** Enter in to config mode

1. line console 0 🡪cse(config-line)# 🡪 here 0 indicating port is 1 st one
2. run command>password <enter password> 🡪ksv123
3. 🡪 enter another password. (setting password to line console) 🡪 which is not equal to palin and secreat password
4. Now use command>login
5. Exit🡪 New we are at propagation mode
6. Exit 🡪 got to usermode
7. And it asks for user>Access verification
8. And asks for password > enter line console password.9
9. Line config to remove password 🡪 just say no password.

>No enable secreat <your password>